**Top Air Opaque**

**Directions for Use**

* Shake well before applying.
* Clean surface of any residual wax or greasy film.
* Roughen metal surface for bonding enhancement.
* Apply after boil out on cool, dry metal surface.
* Paint on thin and add thinner as needed to keep thinned.

**Enhancing Bond**:

* Sprinkle a bit of **Top Paqubond** powder in with **Top Air Opaque** on a dappen dish and mix thoroughly.
* As mixture it is thickening, brush onto metal surface and allow curing.

**Precautions**:

* Keep container capped. If **Top Air Opaque** solidifies add **Top Air Opaque thinner** as necessary, let stand for three days and then shake and stir to reformat the thin liquid paste.