**Top Marker**

**Directions for Use**

**Preparation:**

* For use on models, coat surface using Top Sealer/Top Hardener, to avoid penetration of the solution into the stone.
* Shake well before using.
* Use brush to spot liquid on suspected contact areas.
* For crowns and bridges, apply to stump and fit attachment.
* To detect occlusal or basal contacts, paint respective plaster.
* Press firmly to transfer marker.
* Separate parts to inspect proximity markings.
* Wash off with running water when proper fitment is confirmed.

**Precautions**:

* Close container immediately after each application.
* Consistency can be adjusted by adding **Top Thinner**.
* For use on models, coat surface using Top Sealer/Top Hardener, to avoid penetration of the solution into the stone.