**Die Spacer**

**Directions for Use**

**Preparation:**

* Clean and dry die surface.
* Shake container well, mix all pigments thoroughly.
* If **Die Spacer** is viscous, add thinner for a free flow.
* Using smooth, even brush strokes, allow 30 seconds to 1 minute between coats for drying time.

**Application**

* When die is ready to accept wax, lubricate the surface before pouring wax.