**Top Die Lube**

**Directions for Use**

**Preparation:**

* Clean die, remove debris and visible dust.
* Apply thin coat consistently and completely by spray or brush, including top edges and rim of die.
* Check to make sure **Top Die Lube** covers margins.
* Brush out puddles or excess thickness.
* Air blow and shake upside down to remove excess liquid.
* Let stand one or two minutes before filling with wax.
* Wax up past rim of die.