**Top Vacudeb**

**Directions for Use**

**Preparation:**

* Shake well before using.
* Clean die, removing debris and visible dust and let dry.
* Apply sparingly with brush or misting spray applicator.
* Apply to all surfaces with a smooth, even coat.
* Verify indentions and narrow fissures are coated.
* Shake to remove excess liquid.
* After drying, pour investment into die with gentle vibration.

**Precautions**:

* Close container immediately after each application.
* Contains alcohol. Do not inhale and use mask when applying.